<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="78" y2="0" width="0" layer="20"/>
<wire x1="78" y1="0" x2="78" y2="77" width="0" layer="20"/>
<wire x1="78" y1="77" x2="0" y2="77" width="0" layer="20"/>
<wire x1="0" y1="77" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="LilyPad-Wearables">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of sewable boards, textile footprints, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED2" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED3" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED4" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED5" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED6" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED7" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED8" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED9" library="LilyPad-Wearables" package="LED-1206" value=""/>
<element name="LED10" library="LilyPad-Wearables" package="LED-1206" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED7" pad="A"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED6" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="LED10" pad="C"/>
<contactref element="LED9" pad="C"/>
<contactref element="LED8" pad="C"/>
<contactref element="LED7" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED6" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="LED4" pad="C"/>
<contactref element="LED5" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
